> 20.5 | AT^SDPORT Delete a Port Configuration

> The AT^SDPORT write command removes a parallel port. The pins of the port remain open and can be added to a new port.
> Syntax

> Test Command AT^SDPORT=?
> Response(s)
> (list of supported <port_id>s)
> OK

> Write Command AT^SDPORT=<port_id>
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <port_id>(num)

> ID of the port to be closed