> 7.13 | ATS6 Set pause before blind dialing

> Syntax

> Read Command ATS6?
> Response(s)
> <n>
> OK

> Write Command ATS6=<n>
> Response(s)
> OK
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | - | + | + | - | - |  |  | - | + | -

> Command Description
> No effect for GSM.
> Parameter Description

> <n>(num)(&W)(&V)

> 000(&F)...255