> 23.7 | Summary of Unsolicited Result Codes (URC)

> Table 23.10: | Summary of Unsolicited Result Codes (URC)

> AT Command | URC
> Configuration Commands
> AT+CFUN | ^SYSSTART
> AT+CFUN | ^SYSSTART CHARGE ONLY MODE
> AT^SMSO | ^SHUTDOWN
> AT^SCFG | ^SCFG: "AutoExec", <AutoExecState>, <AutoExecType>, <AutoExecIndex>, <AutoExecMode>, <AutoExecATC>
> AT^SCFG | ^SYSSTART AIRPLANE MODE
> Status Control Commands
> AT+CMER | +CIEV: <indDescr>, <indValue>1[, <indValue>2][, <indValue>[,...]]
> AT^SIND | +CIEV: <indDescr>, <indValue>
> AT^SIND | +CIEV: <indDescr>, <adnEntry>, <adnNumber>, <adnType>, <adnText> +CIEV: <indDescr>, "READY"
> AT^SIND | +CIEV: <indDescr>, <indValue>, <vmCounter>
> AT^SIND | +CIEV: <indDescr>, <indValue>, <eonsOperator>, <servProvider>
> AT^SIND | +CIEV: <indDescr>, <nitzUT>, <nitzTZ>, <nitzDST>
> AT^SIND | +CIEV: <indDescr>, <indValue>, <lstaEdv>, <lstaRssi>
> AT^SIND | +CIEV: <indDescr>, <indValue>, <lstaNo>, <lstaMax>, <lstaMin>, <lstaMean>, <lstaVar>
> Call related Commands
> AT^SLCC | if the list of current calls is empty: ^SLCC: if one or more calls are currently in the list: ^SLCC: <idx>, <dir>, <stat>, <mode>, <mpty>, <traffic channel assigned>[, <number>, <type>[, <alpha>]] [^SLCC: <idx>, <dir>, <stat>, <mode>, <mpty>, <traffic channel assigned>[, <number>, <type>[, <alpha>]]] [... ] ^SLCC:
> AT+CRC | RING
> AT+CRC | +CRING: <type>
> Network Service Commands
> AT+CREG | +CREG: <stat>
> AT+CREG | +CREG: <stat>[, <lac>, <ci>]
> AT^SALS | ^SALS: <line>
> Supplementary Service Commands
> AT^SACM | +CCCM: <ccm>
> AT+CCWA | +CCWA: <calling number>, <type of number>, <class>, , <CLI validity>
> AT+CCWA | ^SCWA:
> AT+CLIP | +CLIP: <number>, <type>[, , [, [<alpha>][, <CLI validity>]]]
> AT+COLP | +COLP: <number>, <type>
> AT+CSSN | +CSSI: <code 1>
> AT+CSSN | +CSSU: <code 2>
> AT+CUSD | +CUSD: <m>[<str_urc>[<dcs>]]
> Internet Service Commands
> AT^SISR | ^SISR: <srvProfileId>, <urcCauseId>
> AT^SISW | ^SISW: <srvProfileId>, <urcCauseId>
> Internet Service URC "^SIS" | ^SIS: <srvProfileId>, <urcCause>[, [<urcInfoId>][, <urcInfoText>]]
> GPRS Commands
> AT+CGREG | +CGREG: <stat>
> AT+CGREG | +CGREG: <stat>, <lac>, <ci>
> Short Message Service (SMS) Commands
> AT+CNMI | +CMTI: <mem3>, <index>
> AT+CNMI | +CMT: <length><CR><LF><pdu>
> AT+CNMI | +CMT: <oa>, <scts>[, <tooa>, <fo>, <pid>, <dcs>, <sca>, <tosca>, <length>]<CR><LF><data>
> AT+CNMI | +CBM: <length><CR><LF><pdu>
> AT+CNMI | +CBM: <sn>, <mid>, <dcs>, <page>, <pages><CR><LF><data>
> AT+CNMI | +CDS: <length><CR><LF><pdu>
> AT+CNMI | +CDS: <fo>, <mr>[, <ra>][, <tora>], <scts>, <dt>, <st>
> AT+CNMI | +CDSI: <mem3>, <index>
> AT^SMGO | ^SMGO: <mode>
> SIM related Commands
> AT^SCKS | ^SCKS: <SimStatus>
> AT^SSET | ^SSIM READY
> Remote SIM Access (RSA) Commands
> AT^SRSA | ^SRSA: <devId>, <sapRole>, <connState>
> AT^SRSM | ^SRSM: <RsaDevId>, <RsaMsgId>[, <RsaMsgData>[, <RsaMsgLen>[, <RsaMsgRc>]]]
> SIM Application Toolkit (SAT) Commands
> ^SSTN | ^SSTN: <cmdType>
> ^SSTN | ^SSTN: <cmdTerminateValue>
> ^SSTN | ^SSTN: 254
> ^SSTN | ^SSTN: 255
> Hardware Related Commands
> AT+CALA | +CALA: [<text>]
> AT^SBC | ^SBC: Undervoltage
> AT^SBC | ^SBC: Overvoltage warning
> AT^SBC | ^SBC: Overvoltage shutdown
> AT^SCTM | ^SCTM_A: <m>
> AT^SCTM | ^SCTM_B: <m>
> AT^SRADC | ^SRADC: <ch>, <count>, <value>[, <value>[, <value>[, <value>[, <value>[, <value>[, <value>[, <value>[, <value>[, <value>[, <value>]]]]]]]]]]
> GPIO Commands
> AT^SCPOL | ^SCPOL: <io_id>, <value>
> AT^SCCNT | ^SCCNT: <time>
> AT^SSCNT | ^SSCNT: <pulse>