> 3.6 | AT+CPAS Mobile equipment activity status

> The AT+CPAS execute command indicates the activity status of the ME.
> Syntax

> Test Command AT+CPAS=?
> Response(s)
> +CPAS: (list of supported<pas>s)
> OK

> Exec Command AT+CPAS
> Response(s)
> +CPAS: <pas>
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <pas>(num)

> 0
> Ready
> 3
> Incoming call (ringing)
> 4
> Call in progress or call hold