> 19.7.1 | Specifying Delay Time for I²C

> The parameters <delayOne> and <delayTwo> are depending on the I²C device connected to the TC65. If the delay times set with <delayOne> and <delayTwo> are not adequate the connected I²C device might not be able to answer.
> The following figures are provided to assist you in specifying appropriate values for both parameters. All delays are relative to the data transfer rate. To calculate the delay use the formula and the values given below.

> Figure 19.1: Formula for calculating the delay

> Table 19.2: | Values for calculating the delay

> Parameter | Values
> Delay value | Value set with parameter <delayOne> or <delayTwo>
> Master clock | 13 MHz
> Default data transfer rate | 400 bps
> User data transfer rate | Value selected with subparameter data transfer rate within <basicConfiguration>, for example 100 kbps or 400 kbps
> Delay_min for Write | 7.4 µs at 100 kbps 2.0 µs at 400 kbps
> Delay_min for Read | 9.9 µs at 100 kbps 2.6 µs at 400 kbps

> Figure 19.2: Delay time on I²C after Write

> Figure 19.3: Delay time on I²C after Read