> 16.4 | AT^SSTR SAT Response

> The TA is expected to acknowledge the AT^SSTGI response with AT^SSTR to confirm that the Proactive Command has been executed. AT^SSTR will also provide any user information, e.g. a selected menu item.
> Syntax

> Test Command AT^SSTR=?
> Response(s)
> ^SSTR:(list of supported <state>s), (list of supported <cmdType>s)
> OK

> Read Command AT^SSTR?
> Response(s)
> ^SSTR: <state>, <cmdType>
> OK

> Write Command AT^SSTR=<cmdType>, <status>[, <inputNumber>][, <inputString>]
> Response(s)
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <state>(num)

> TC65 Remote-SAT interface states
> 0
> RESET
> 1
> OFF
> 2
> IDLE
> 3
> PAC
> 4
> WAIT

> <cmdType>(num)

> Number related to Proactive Command or event type according to GSM 11.14 [27].

> <status>(num)

> Command status return regarding the type of action that has taken place, e.g. action performed by the user. Values are in accordance with GSM 11.14 [27].

> <inputNumber>(num)

> Response number entered by user

> <inputString>(str)

> Response string entered by user