> 20.4 | AT^SCPORT Port Configuration

> With AT^SCPORT a group of maximum 10 pins can be configured to act as a parallel port, which can be controlled with a single AT command. A pin can only be added once to a port, and only to a port. The first, i.e. left most parameter, corresponds to the port's LSB.
> All pins of a port must be set to the same direction (input or output). See AT^SCPIN.
> Syntax

> Test Command AT^SCPORT=?
> Response(s)
> OK

> Write Command AT^SCPORT=<pin_id>1[, <pin_id>2[, <pin_id>3[, <pin_id>4[, <pin_id>5[, <pin_id>6[, <pin_id>7[, <pin_id>8[, <pin_id>9[, <pin_id>10]]]]]]]]]
> Response(s)
> ^SCPORT: <port_id>
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <port_id>(num)

> Assigned port

> <pin_id>(num)

> Pin ID of the xth pin of this port
> See AT^SCPIN for possible pin value.