> 23.6 | Factory Default Settings Restorable with AT&F

> Table 23.9: | Factory Default Settings Restorable with AT&F

> AT Command | Factory Defaults
> Configuration Commands
> ATQ | <n>=0
> ATV | <value>=1
> ATX | <value>=4
> AT\V | <value>=1
> AT+CFUN | <fun>=1
> AT+CMEE | <errMode>=0
> AT+CSCS | <chset>="GSM"
> AT^SM20 | <CallMode>=1, <CmgwMode>=1
> AT^SCFG | <tcpBufSize>="5200", <tcpIrt>="3", <tcpMr>="10", <tcpOt>="6000", <tcpWithUrc>="on"
> Status Control Commands
> AT+CMER | <mode>=0, <keyp>=0, <disp>=0, <ind>=0, <bfr>=0
> AT+CIND | <mode>=1
> ATS18 | <n>=0
> Serial Interface Control Commands
> AT\Q | <n>=0
> AT&C | <value>=1
> AT&D | <value>=2
> AT&S | <value>=0
> ATE | <value>=1
> AT+IFC | <TEflowcontrol>=0, <TAflowcontrol>=0
> AT+ILRR | <value>=0
> AT^STPB | <n>=0
> Call related Commands
> ATS0 | <n>=000
> ATS6 | <n>=000
> ATS7 | <n>=060
> ATS8 | <n>=0
> ATS10 | <n>=002
> AT+CBST | <speed>=7, <name>=0, <ce>=1
> AT+CRLP | <iws>=61, <mws>=61, <T1>=78, <N2>=6
> AT^SLCC | <n>=0
> AT+CR | <mode>=0
> AT+CRC | <mode>=0
> Network Service Commands
> AT+COPS | <format>=0
> AT+CREG | <n>=0
> AT^SALS | <view>=0, <line>=1
> Supplementary Service Commands
> AT^SACM | <n>=0
> AT+CLIP | <n>=0
> AT+CSSN | <n>=0, <m>=0
> AT+CUSD | <n>=0
> GPRS Commands
> AT+CGAUTO | <n>=3
> AT+CGREG | <n>=0
> AT+CGSMS | <service>=3
> AT^SGAUTH | <auth>=1
> ATS0 | <n>=000
> FAX Commands
> AT+FCLASS | <n>=0
> Short Message Service (SMS) Commands
> AT+CMGF | <mode>=0
> AT+CNMI | <mode>=0, <mt>=0, <bm>=0, <ds>=0, <bfr>=1
> AT+CSCB | <mode>=0, <mids>=" ", <dcss>=" "
> AT+CSDH | <show>=0
> AT+CSMP | <fo>=17, <vp>=167, <dcs>=0, <pid>=0
> AT+CSMS | <service>=0
> AT^SMGO | <n>=0
> AT^SSCONF | <ra>=0
> AT^SSDA | <da>=0
> AT^SSMSS | <seq>=0
> SIM related Commands
> AT^SCKS | <mode>=0
> AT^SSET | <n>=0
> Phonebook Commands
> AT+CPBS | <storage>="SM"
> AT^SPBS | <internal-counter>=0
> Audio Commands
> AT+VTD | <duration>=1
> Hardware Related Commands
> AT^SCTM | <n>=0
> AT^SSPI | <connectionState>=0, <delayOne>=0, <delayTwo>=0
> Miscellaneous Commands
> ATS3 | <n>=013
> ATS4 | <n>=010
> ATS5 | <n>=008