> 19.7.6 | Example: Transfer and Response Messages on SPI

> The following examples shall illustrate the message structure and write/read procedures explained in Section 19.7.3.2, Structure of Messages on the SPI. Blanks are inserted only to better visualize frame elements. In practice no blanks are allowed.

> <0 00 0000 11 22 33> | Transfer Message: The master writes 3 bytes.
> {0 +} | Response Message: Transmission successful.

> <1 00 0010> | Transfer Message: The master requests to read 16 bytes from the slave. Read Offset is zero, therefore, reading starts from the first byte.
> {1 + 11 22 33 44 ... FF 00} | Response Message: Reading data successful.

> <2 03 0008> | Transfer Message: The master requests to read 8 bytes from the slave. Read Offset is 3, therefore, reading starts from the fourth byte.
> {2 + 44 55 66 77 88 99 AA BB} | Response Message: Reading data successful.

> <3 03 0004 11 22 33 44 55 66> | Transfer Message: The master writes 6 bytes and requests to read 4 bytes from the slave. Read Offset is 3, therefore, reading starts from the fourth byte.
> {3 + AA BB CC DD} | Response Message: Reading and writing data successful.