> 3.5.2 | Installing the SMTK Environment

> Before you start the installation please make sure all applications, especially the IDEs are closed.

> 1. | Insert the CD, start setup.exe. When the dialog box appears press the Next button.

> 2. | You will be asked to read the license agreement. If you accept the agreement, press Yes to continue with the installation.

> 3. | A file including special information about the installation and use of the SMTK is shown. Press Next to continue.

> 4. | You will be asked to enter the path name where Eclipse 3.0.1, 3.0.2, 3.1.0, 3.1.1, 3.1.2 or 3.2.x1 is installed. Please type in the folder where Eclipse with the ME plugin is installed and press Next. If you have not installed Eclipse or do not want to integrate the SMTK into Eclipse, please press Next without typing in a selected folder.

> 5. | The installation software checks for the Java SDK. If there is no SDK on the system the installation procedure now offers to install the provided JDK. If this step is refused, the setup process will not continue because a properly installed JDK is mandatory for using the SMTK environment.

> 6. | At this point, the installation software checks for a Java IDE to be integrated with the SMTK. A Java IDE is not necessary to use the SMTK. The IDE installation can be done at any time even if the SMTK is already installed. To integrate the SMTK into the Java IDE run the SMTK setup program in maintenance mode again. However, you can continue the setup procedure and install the IDE installation later or cancel the setup program at this stage and restart it after installing one of the supported Java IDEs. In case you wish to install a Java IDE please follow the instructions below and in Section 3.5.3. If no installed IDE is found the SMTK offers to install NetBeans IDE 5.0 and NetBeans Mobility package 5.0 (NetBeans 5.5.1 and NetBeans Mobility package 5.5.1 is distributed with TC65 CD). Alternatively, you can install the SUN IDE by following the instructions in Section 3.5.3.

> 7. | If the SDK and one or more Java IDEs are found, you will be asked to choose which IDE you want integrated into the development environment. Once an IDE has been found and selected, press Next to continue. Ensure that your Java IDE is closed.

> 8. | Select the folder where the SMTK will be installed. A folder will be suggested to you but you may browse to select a different one.

> 9. | Choose the path that SMTK will appear under in the Start Menu.

> 10. | In the next installation dialog box you will be asked to to create a Dial-up Network connection for on-device debugging. This Dial-up Network connection can be configured either for the Standard 119200 bps Modem integrated in Windows or the USB modem. As a result, a Dial-up Network connection will be created named "IP connection for remote debugging" (the connection will be available after the entire installation of the SMTK environment).

> - | If a Dial-up Network connection named "IP connection for remote debugging" is already available for another Siemens IMP-NG product, you can choose to reconfigure the existing connection by pressing Yes or leave it unchanged by pressing No.

> - | If you have selected Yes or if there was no on-device connection before, check either "Serial COM port for using the standard modem installation" or "USB COM port for using the USB modem installation".

> - | If you have chosen the Standard 119200 bps Modem select the COM port number, click Next. In the resulting dialog box select the baud rate and click Next again.

> - | If you have chosen the USB modem the available USB modems will be listed. Choose the "Siemens AG WM USB Modem" and click Next.

> Note: You can reconfigure the COM port for the Dial-Up Network connection any time after the installation by starting the SMTK setup in maintenance mode and selecting “Repair” mode.

> 11. | Select the IP address used for IMP-NG on-device debugging and the UPD port number used for switching the Java “System.out” direction to serial port output.

> 12. | A brief summary of all entries made is shown. Press Next to continue.

> 13. | A status message box informs you that the Module Exchange Suite (MES) will be installed now. A separate MES setup wizard opens. Please follow the setup wizard’s instructions.

> 14. | All necessary files will be copied from the CD into the target folder.

> 15. | This is the final step. Again, a listing of all installed components appears. Please press Fin ish to end the installation.

> How to use the "Modify" or "Repair" mode:
> To open either mode click Control Panel → Add or Remove Programs. Select SMTK installation and press “Modify” or “Repair”:
> Please keep in mind, that Windows system requires the same location of the installation CD, if you like to use “Modify” or “Repair” for the SMTK installation. The installer is searching for *.msi file and an installer message box will pop up, telling the user to locate the installation CD in the corresponding drive and path. If the installation CD is not located on the displayed drive and path, please insert the CD or copy the CD contents into the required location (drive and path).
> Note for installing the SMTK environment on Windows 2000 systems:
> Please delete all modems with device name "Standard 19200 bps Modem" before installing the SMTK environment on a Windows 2000 system, because this modem device is used during automatic modem installation and on-device debugging.

> 1
> Supported only for TC65