> 2.18.1 | Initialization of Remote SAT

> This section comprises the subsections Description, Used AT Commands, Flow Chart, Hints and Example. To move to these subsections please use the Navigation Frame or the appropriate buttons on the toolbar.

> 2.18.1.1 | Description

> This chapter describes the initialization of Remote SAT. Usually an SMS is send to the network provider containing service requests, e.g. send latest news. Please set follow parameters to receive messages: the SMS text mode (AT+CMGF=1), active display of an URC on every received SMS (AT+CNMI=1,1). In case of more detailed header information use (AT+CSDH=1).

> 2.18.1.2 | Used AT commands

> Command | Explanation
> AT+CMGF | Select SMS message format
> AT+CNMI | New SMS message indications
> AT+CSDH | Show SMS text mode parameters

> For further details about the commands see [2].

> 2.18.1.3 | Flow chart

> Figure 172: RSAT initialization

> 2.18.1.4 | Hints

> Not applicable.

> 2.18.1.5 | Example

> Not applicable.