> 2.1 | Technical Specification

> • | USB 2.0 Full Speed compatible (12 Mbit/s)

> • | Compliant with “Universal Serial Bus Specification Revision 2.0”

> • | Self-powered device, control via USB host only (for details see [1])

> • | Supports Multiplex mode, i.e. the USB interface can be partitioned into virtual channels

> • | Supported configurable IDs: Vendor ID, Product ID and Serial number

> The USB interface is primarily intended for use as command and data interface and for downloading firmware. The USB I/O-pins are capable of driving the signal at min 3.0V. They are 5V I/O compliant.