> 3.5 | User profile settings

> When the WinMux driver is started, the module will be initialized to use the following settings on multiplexer channel 1:

> • | Baud rate as specified on the Multiplexer Property page

> • | AT&S0: DSR always on. Not applicable to XC18.

> • | AT\Q3: Hardware flow control

> • | AT+ICF=3: Sets interface mode 8N1. This command works only on modules supporting different interface modes (TC35i, TC63, TC65, MC75, AC65, AC75, XT65, XT75). The resulting ERROR on modules without support of the AT+ICF command is ignored by the WinMux driver.

> This way, the initialization sequence will override, on multiplexer channel 1, any other settings of AT&S, AT\Qn and AT+ICF you may have stored to the user profile with AT&W before starting the multiplexer. After restart without multiplexer, the user profile will be loaded again with all your individual settings.