> 8.12 | AT^SMONG GPRS Monitor

> The AT^SMONG command supplies GPRS specific cell information. There are two ways to retrieve the information: once on request by using the execute command or automatically every <period> seconds by using the write command. To stop the periodic presentation type "AT" or "at".
> Syntax

> Test Command AT^SMONG=?
> Response(s)
> ^SMONG:(list of supported <table>s), (list of supported <period>s)
> OK
> ERROR
> +CME ERROR

> Exec Command AT^SMONG
> Response(s)
> GPRS Monitor
> Cell Info Table (see: Section 8.12.1, AT^SMONG Cell Info Table)
> OK
> ERROR
> +CME ERROR

> Write Command AT^SMONG=<table>[, <period>]
> Response(s)
> ^SMONG: GPRS Monitor
> Cell Info Table (see: Section 8.12.1, AT^SMONG Cell Info Table)
> OK
> ERROR
> +CME ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | - | -

> Parameter Description

> <table>(num)

> 1
> Cell Info Table

> <period>(num)

> Display period in seconds
> If <period> is omitted the cell data will be presented only once on a single line (as if Execute command was issued).
> If <period> is given, the cell data will be listed repeatedly on 10 data lines. Every 10th data line is followed by the header, simply to repeat the column titles.
> 1...100
> Notes

> • | For compatibility with earlier products and to support legacy applications, often any input character will stop the periodic output of the write command. But since this applies only in certain cases (depending on the settings of AT+IPR and AT+CMUX), it is recommended to always use "at" or "AT".

> • | If the ME is Java controlled, periodic retrieval of cell information using the write command AT^SMONG=<table>,<period> is not supported. If periodic cell information is required simply repeat the execute commands at regular intervals.