> 10.1.2 | Example: GPRS connection profile

> at^sics=0,conType,GPRS0 | Select connection type GPRS0.
> OK
> AT^SICS=0,inactTO,"0" | Inactivitiy timeout = 0 (default).
> OK
> AT^SICS=0,dns1,"193.254.160.1" | IP address of Primary DNS server.
> OK
> AT^SICS=0,authMode,"PAP" | Authentication protocol PAP (default).
> OK
> AT^SICS=0,passwd,t-d1 | Password for GPRS services provided by the German operator T-D1.
> OK
> AT^SICS=0,apn,"internet.t-d1.de" | APN to access the GPRS services provided by the German operator T-D1.
> OK