> 11.17 | ATA Manual response to a network request for PDP context activation

> The V.250 ATA command may be used to accept a network request for a PDP context activation announced by the unsolicited result codes "RING" or "+CRING: GPRS". The MT responds with CONNECT, enters V.250 online data state and follows the same procedure as it would after having received a AT+CGANS=1 with no <L2P> or <cid> values specified.
> If you try to answer a request which is no longer present or which is already answered by another instance, NO CARRIER is returned.
> Syntax

> Exec Command ATA
> Response(s)
> CONNECT
> NO CARRIER

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | + |  | + | + | + | + | + | + |  |  | - | - | +