> 2.3 | AT&W Stores current configuration to user defined profile

> AT&W stores the currently set parameters to a user defined profile in the non-volatile memory.
> Syntax

> Exec Command AT&W[<value>]
> Response(s)
> OK
> ERROR/+CME ERROR <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <value>(num)

> [0]
> Number of profile
> Notes

> • | The user defined profile will be restored automatically after power-up. Use ATZ to restore user profile and AT&F to restore factory settings. Until the first use of AT&W, ATZ works as AT&F.

> • | AT&W stores all global settings and the current local settings of the interface, on which the command is executed.

> • | A list of parameters stored to the user profile can be found in Section 23.5, AT Command Settings storable with AT&W.