> 3.4 | Set up Java Development Environment with Eclipse IDE (Quick Start-up)

> Please complete the following steps to set up your Eclipse Java development environment:
> Step 1:
> Install JDK 1.4.2_09
> → JDK 1.4\j2sdk-1_4_2_09-windows-i586-p.exe
> For TC65 install JDK 1.5.0_07 , if no JDK 1.5 or higher is installed on your machine.
> Step 2:
> Install Eclipse 3.1.2
> → Unzip from CD ("\Eclipse\eclipse-SDK-3.1.2-win32.zip") to "C:\Program Files\Eclipse"
> (Installation of Eclipse 3.2.2 to be employed with TC65 is completed in the same way.)
> Step 3:
> Installation Eclipse ME plugin 1.2.3:
> (Installation of Eclipse ME plugin 1.6.8 to be employed with TC65 is completed in the same way)

> - | Start Eclipse IDE

> - | Select the default workspace suggested by Eclipse

> - | Start ME plugin installer using Eclipse menu Help → Software Updates → Find and Install.

> Figure 2: Installation of Eclipse ME-Plugin 1.2.3: Dialog box Feature Updates
> Figure 3: Installation of Eclipse ME-Plugin 1.2.3: Dialog box Updates sites to visit

> - | Select the path where Eclipse ME plugin is located on CD (EclipseMEplugin_123\.....") and select „eclipseme.feature_1.2.3_site.zip"

> Figure 4: Installation of Eclipse ME-Plugin 1.2.3: dialog box Search Results

> - | In the dialog box Verification, select Install All.

> - | In the dialog box Install/Update, select Yes to restart Eclipse.

> Figure 5: Installation of Eclipse ME-Plugin 1.2.3: dialog box Restart Eclipse

> - | Eclipse IDE is restarted. Please close Eclipse IDE before continuing with installation of SMTK!

> Step 4:
> Installation of the product’s SMTK:

> - | Start "setup.exe" from CD root path.

> - | Choose the destination folder of Eclipse "C:\Program Files\Eclipse" in the dialog box Select Eclipse Folder.

> - | Select SMTK (e.g. C:\Program Files\Siemens\SMTK) in dialog box Destination Folder.

> - | Use the the dialog box Select COM Port to specify the connection type for on-device debugging and MES transfer (downloading the MIDlet to the module): a) Standard 19200 Modem: Choose the COM port and set the baud rate (e.g. 115200). b) USB modem: Select "Siemens AG WM USB Modem". Note that the USB modem has to be installed previously using Siemens "usbmodem.inf" file.

> - | After that, MES will be installed without further user action. Please wait until setup is complete.

> - | Click Finish in the summary dialog to confirm the completed installation.

> A detailed description of the SMTK installation is given in the following chapters.