> 7.6 | ATD><str> Mobile originated call from active memory using corresponding field

> Syntax

> Exec Command ATD><str>[<mgsm>];
> Response(s)
> ERROR
> +CME ERROR: <err>
> If no dialtone (parameter ATX2 or ATX4):
> NO DIALTONE
> If busy (parameter setting ATX3 or ATX4):
> BUSY
> If connection cannot be set up:
> NO CARRIER
> When TA returns to command mode after call release:
> OK
> If successfully connected:
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | + |  | + | ± | + | + | ± | ± |  |  | - | - | -

> Command Description
> This command searches the active phonebook for a given string <str> and dials the assigned phone number. The termination character ";" is mandatory since dialing from a phonebook is only supported for voice calls and for sending *# codes of Supplementary Services or other functions.
> Parameter Description

> <str>(str)(+CSCS)

> String type value ("x"), which should equal an alphanumeric field in at least one phonebook entry in the searched memories; used character set should be the one selected with AT+CSCS. <str> can contain escape sequences as described in chapter "Supported character sets".
> <str> must be wrapped in quotation marks (""), if escape sequences or parameter <mgsm> are used or if the alphanumeric strings contains a blank. If not, quotation marks are optional.
> If AT+CSCS is set to "UCS2", with respect to the coding of UCS2-characters only phonebook entries that contain an alphanumeric string with a size less than the half of the parameter <tlength> from AT+CPBW can be dialed.

> <mgsm>(str)

> String of GSM modifiers:
> I Activates CLIR (disables presentation of own phone number to called party)
> i Deactivates CLIR (enables presentation of own phone number to called party)
> Notes

> • | This command may be aborted generally by receiving a character during execution. Abortion is not possible during some states of connection setup such as handshaking.

> • | The command is not applicable to data calls. Any attempt to dial <str> without semicolon ";" causes the result code "NO CARRIER" to appear.

> • | Parameter <mgsm> only if no *# code is within the dialing string.