> 7.16 | ATS10 Set disconnect delay after indicating the absence of data carrier

> Syntax

> Read Command ATS10?
> Response(s)
> <n>
> OK

> Write Command ATS10=<n>
> Response(s)
> OK
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | - | + | + | - | - |  |  | - | + | -

> Command Description
> This parameter setting determines the amount of time, that the TA remains connected in absence of a data carrier. If the data carrier is detected before disconnect, the TA remains connected.
> Parameter Description

> <n>(num)(&W)(&V)

> number of tenths of seconds of delay
> 001...2(&F)...254