> 13.26 | AT^SSCONF SMS Command Configuration

> AT^SSCONF controls details of some SMS releated commands. Please note that AT^SSCONF settings are stored volatile, i.e. after restart or reset the default values will be restored.
> Syntax

> Test Command AT^SSCONF=?
> Response(s)
> ^SSCONF:list of supported <ra>s
> OK

> Read Command AT^SSCONF?
> Response(s)
> ^SSCONF:<ra>
> OK

> Write Command AT^SSCONF=<ra>
> Response(s)
> OK

> PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <ra>(num)

> Display recipient address
> [0](&F)
> TC65 does not display <ra> and <tora>. These parameters are used with the result codes of AT+CMGL, AT^SMGL, AT+CMGR, AT^SMGR and the URC "+CDS".
> 1
> TC65 displays <ra> and <tora>.