> 13.14 | AT+CSCB Select Cell Broadcast Message Indication

> The test command returns the supported modes as a compound value.
> The write command selects which types of CBMs are to be received by the ME.
> Syntax

> Test Command AT+CSCB=?
> Response(s)
> +CSCB: (list of supported <mode>s)
> OK

> Read Command AT+CSCB?
> Response(s)
> +CSCB: <mode>, <mids>, <dcss>
> OK

> Write Command AT+CSCB=<mode>[, <mids>[, <dcss>]]
> Response(s)
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.05 |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <mode>(num)

> Message mode
> 0(&F)
> Accept messages that are defined in <mids> and <dcss>
> 1
> Forbid messages that are defined in <mids> and <dcss>

> <mids>(str)

> Cell Broadcast Message ID specification
> [““](&F)
> default value of this parameter is empty string, and it means that no CBM identifiers are specified.

> • | For <mode>=0: Six different possible combinations of CBM IDs (e.g. "0,1,5,320-478,922,2000-3000"). In certain configurations, e.g. if using SIMs that contain data in Elementary File EF-CBMID (Cell Broadcast Message Identifier for Data download) less than six combinations may be available. To access a SIM's Elementary File data refer to command AT+CRSM.

> • | For <mode>=1: One CBM ID or range of IDs (e.g. "320-478").

> <dcss>(str)

> CBM data coding scheme specification
> [““](&F)
> default value of this parameter is empty string
> All different possible combinations of CBM data coding schemes (e.g. "0-3,5"). Using default empty string leads to get all CBMs independent of their dcss.
> A given <dcss> replaces any former value and is used for consecutive requests.