> 6.8 | AT+CGSN Request International Mobile Equipment Identity (IMEI)

> AT+CGSN delivers the International Mobile Equipment Identity (IMEI). Command is identical with: AT+GSN.
> Syntax

> Test Command AT+CGSN=?
> Response(s)
> OK

> Exec Command AT+CGSN
> Response(s)
> <sn>
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <sn>(str)

> International Mobile Equipment Identity (IMEI) used to identify a GSM mobile equipment to the GSM network