> 7.5 | ATD><n> Mobile originated call from active memory using index number

> Syntax

> Exec Command ATD><n>[<mgsm>];
> Response(s)
> ERROR
> +CME ERROR: <err>
> If no dialtone (parameter ATX2 or ATX4):
> NO DIALTONE
> If busy (parameter setting ATX3 or ATX4):
> BUSY
> If connection cannot be set up:
> NO CARRIER
> When TA returns to command mode after call release:
> OK
> If successfully connected:
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | + |  | + | ± | + | + | ± | ± |  |  | - | - | -

> Command Description
> TA attempts to set up an outgoing call to the stored number. The termination character ";" is mandatory since dialing from a phonebook is only supported for voice calls and for sending *# codes of Supplementary Services or other functions.
> Parameter Description

> <n>(num)

> Integer type memory location in the range of locations available in the selected memory, i.e. the index number returned by AT+CPBR.

> <mgsm>(str)

> String of GSM modifiers:
> I Activates CLIR (disables presentation of own phone number to called party)
> i Deactivates CLIR (enables presentation of own phone number to called party)
> Notes

> • | This command may be aborted generally by receiving a character during execution. Abortion is not possible during some states of connection setup such as handshaking.

> • | The command is not applicable to data calls. Any attempt to dial a data call number from <n> causes the result code "NO CARRIER" to appear.

> • | Parameter <mgsm> only if no *# code is within the dialing string.