> 2.6 | ATX Set CONNECT result code format and call monitoring

> ATX determines whether or not the TA detects the presence of dial tone and busy signal and whether or not TA transmits particular result codes.
> Syntax

> Exec Command ATX[<value>]
> Response(s)
> OK
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <value>(num)(&W)(&V)

> [0]
> CONNECT result code only returned, dial tone and busy detection are both disabled.
> 1
> CONNECT <text> result code only returned, dial tone and busy detection are both disabled.
> 2
> CONNECT <text> result code returned, dial tone detection is enabled, busy detection is disabled.
> 3
> CONNECT <text> result code returned, dial tone detection is disabled, busy detection is enabled.
> 4(&F)
> CONNECT <text> result code returned, dial tone and busy detection are both enabled.