> 2.12 | AT+CMEE Mobile Equipment Error Message Format

> AT+CMEE controls the format of the error result codes that indicates errors related to TC65 functionality. Format can be selected between plain "ERROR" output, error numbers or verbose "+CME ERROR: <err>" and "+CMS ERROR: <err>" messages.
> Possible error result codes are listed in Table 2.4, General "CME ERROR" Codes (GSM 07.07)Table 2.5, General "CME ERROR" Codes (SIEMENS)Table 2.6, GPRS related "CME ERROR" Codes (GSM 07.07) and Table 2.8, SMS related "CMS ERROR" Codes (GSM 07.05).
> In multiplex mode (refer AT+CMUX) the setting applies only to the logical channel where selected. The setting on the other channels may differ.
> Syntax

> Test Command AT+CMEE=?
> Response(s)
> +CMEE: (list of supported<errMode>s)
> OK

> Read Command AT+CMEE?
> Response(s)
> +CMEE: <errMode>
> OK

> Write Command AT+CMEE=<errMode>
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <errMode>(num)(&W)(&V)

> 0(&F)(D)
> Disable result code, i.e. only "ERROR" will be displayed.
> 1
> Enable error result code with numeric values.
> 2
> Enable error result code with verbose (string) values.
> Example
> To obtain enhanced error messages it is recommended to choose <errMode>=2.

> AT+CMEE=2
> OK