> 2.2 | Technical Requirements for Using TC65 Terminal

> • | Computer running Microsoft® Windows XP™ and Microsoft® Windows Vista™

> • | 1.8V or 3.0V SIM card

> • | 8 to 30 Volts power supply unit

> • | RS-232 cable (for high data rates = 1.5m)

> • | UART capable of data rates up to 460800 bps. Usually this requires an appropriate serial adapter to be installed on the computer.

> • | RF antenna

> • | Audio handset

> • | Customized mating connector for the IO interface connector type Micro Mate-N-LOK.

> • | Terminal program to control the COM port, for example Windows HyperTerminal.

> • | Access to a GSM/GPRS network providing support of the authentication protocol PAP, CHAP or MS-CHAP. The GPRS settings of your service provider should be at hand. Please contact your service provider or follow the link below to obtain all required information.

> http://www.gsmworld.com/technology/gprs/operators.shtml