> 10.14.5 | Socket client sends data via TCP connection with URCs

> The example uses service profile 0 configured for Socket service and TCP.

> AT^SISO=0 | The host opens service profile 0.
> OK
> ^SISW: 0,1 | Socket service is ready for upload.
> AT^SISW=0,10 | The host requests to write 10 bytes.
> ^SISW: 0,10,10 | Response that 10 bytes can be sent and are unacknowledged.
> 0123456789
> OK
> ^SISW: 0,1 | The URC indicates that the Socket service is ready to transfer more data. Data of the last AT^SISW command are transferred to the remote host.
> AT^SISW=0,10,1 | The host requests to write next 10 bytes and enables the end-of-data flag to notify that these are the last 10 bytes of the session.
> ^SISW: 0,10,20 | Response that the service accepts 10 bytes and this data and the previously sent data are unacknowledged.
> 0123456789
> OK
> ------ | Waiting for URC.
> ^SISW: 0,2 | Data transfer has been finished.
> AT^SISC=0 | Closing the Socket service.
> OK