> 7.17 | ATO Switch from command mode to data mode / PPP online mode

> Syntax

> Exec Command ATO[<n>]
> Response(s)
> If connection is not successfully resumed:
> NO CARRIER
> or
> TA returns to data mode from command mode
> CONNECT <text>
> Note: <text> output only if ATX parameter setting with value > 0.

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | ± | + | + | - | - |  |  | - | - | -

> Command Description
> ATO is the corresponding command to the +++ escape sequence: When you have established a CSD call or a GPRS connection and TA is in command mode, ATO causes the TA to resume the data or GPRS connection and takes you back to data mode or PPP online mode.
> Parameter Description

> <n>(num)

> [0]
> Switch from command mode to data mode