> 4.5 | ATE Enable command echo

> The ATE command determines whether or not the TA echoes characters received from TE during command state.
> Syntax

> Exec Command ATE[<value>]
> Response(s)
> OK

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <value>(num)(&W)(&V)

> [0]
> Echo mode off
> 1(&F)
> Echo mode on
> Notes

> • | In case of using the command without parameter, <value> is set to 0.

> • | When a Java application is running there is no echo available, existing settings are ignored and attempts to change the settings are disregarded.