> 14.6 | AT^SSET Indicate SIM data ready

> After power-up and personalization (PIN entry if required) the ME starts reading data from SIM. The AT^SSET command controls the presentation of the "^SSIM READY" URC which indicates, on the corresponding serial channel, when the ME has finished reading SIM data. See Section 23.1, Restricted access to SIM data after SIM PIN authentication for further detail.
> Syntax

> Test Command AT^SSET=?
> Response(s)
> ^SSET:(list of supported <n>s)
> OK

> Read Command AT^SSET?
> Response(s)
> ^SSET: <n>
> OK
> ERROR
> +CME ERROR: <err>

> Write Command AT^SSET=[<n>]
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Unsolicited Result Code
> ^SSIM READY
> The URC acknowledges to the user that SIM data is accessible.
> Parameter Description

> <n>(num)(&W)(&V)

> URC presentation mode
> 0(&F)
> Disable URC "^SSIM READY" indication.
> 1
> Enable URC "^SSIM READY" indication.