> 22.4 | ATS5 Write command line editing character

> Syntax

> Read Command ATS5?
> Response(s)
> <n>
> OK

> Write Command ATS5=<n>
> Response(s)
> OK
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Command Description
> This parameter setting determines the character recognized by TA as a request to delete the immediately preceding character from the command line.
> Parameter Description

> <n>(num)(&W)(&V)

> command line editing character
> 000...8(&F)...127