> 14.8 | AT+CXXCID Display card ID

> Syntax

> Test Command AT+CXXCID=?
> Response(s)
> OK

> Exec Command AT+CXXCID
> Response(s)
> +CXXCID: <cid>
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Command Description
> TA returns the card identification number in SIM (SIM file EF ICCID, see GSM 11.11 Chap.10.1.1) as string type.
> Note

> • | See also: AT^SCID.