> 10.12 | AT^SISE Internet Service Error Report

> The AT^SISE write command returns the current error status of the specified Internet service profile. If the service profile is not defined or the value is invalid "+CME ERROR" response is returned.
> The error status is identical to the content of the "^SIS" URC last issued.
> If a service fails the commands AT^SISR or AT^SISW will return an error response. However, if the AT^SISE command returns <infoID>=0 it is recommended to use the AT+CEER command because a general GSM/GPRS problem might be the reason.
> Syntax

> Test Command AT^SISE=?
> Response(s)
> OK

> Write Command AT^SISE=<srvProfileId>
> Response(s)
> ^SISE: <srvProfileId>, <infoID>[, <info>]
> OK
> ERROR
> +CME ERROR: <err>

> PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> - |  | + | + | + | + | + | + |  |  | - | - | -

> Parameter Description

> <srvProfileId>(num)

> Internet service profile identifier as defined by AT^SISS <srvProfileId>.
> 0...9

> <infoID>(num)

> Reason for Internet service error. This is a subset of the <urcInfoId>s which can be found in Section 10.13, Internet Service URC "^SIS".
> The value 0 indicates there is no special Internet service error. In this case the application may use AT+CEER to check for general GSM/GPRS problems.

> <info>(str)

> Information text related to <infoID>. This is a subset of the <urcInfoText>s which can be found in Section 10.13, Internet Service URC "^SIS".
> Note

> • | In particular cases, the AT^SISE command may deliver information and warnings. This applies the following services: FTP: Information 2100 POP3: Warnings SMTP: Warnings If an error occurs the information and warning messages are overwritten by error messages.