> 13.19 | AT^SCMR Read Concatenated Short Messages

> The write command returns the message with location value <index> from message storage <mem1> to the TE. If the status of the message is 'received unread', the status in the storage changes to 'received read'. See notes of AT+CMGR.
> Syntax

> Test Command AT^SCMR=?
> Response(s)
> OK

> Write Command AT^SCMR=<index>
> Response(s)
> Output if text mode (AT+CMGF=1) and command successful:
> For SMS-DELIVER
> ^SCMR: <stat>, <oa>, [<alpha>], <scts>[, <tooa>, <fo>, <pid>, <dcs>, <sca>, <tosca>, <length>][, <seq>, <max>, <ieia>, <ref>]
> <data>
> [... ]
> OK
> For SMS-SUBMIT
> ^SCMR: <stat>, <da>, [<alpha>][, <toda>, <fo>, <pid>, <dcs>, [<vp>], <sca>, <tosca>, <length>][, <seq>, <max>, <ieia>, <ref>]
> <data>
> [... ]
> OK
> For SMS-STATUS-REPORT
> ^SCMR: <stat>, <fo>, <mr>, [<ra>], [<tora>], <scts>, <dt>, <st>
> <data>
> [... ]
> OK
> For SMS-Commands
> ^SCMR: <stat>, <fo>, <ct>[, <pid>, [<mn>], [<da>], [<toda>], <length>]
> <data>
> [... ]
> OK
> Output if PDU mode (AT+CMGF=0) and command successful:
> For SMS-SUBMITs and/or SMS-DELIVERs
> ^SCMR: <stat>, [<alpha>], <length>
> <pdu>
> [... ]
> OK
> ERROR
> +CMS ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -