> 16.3 | AT^SSTGI SAT Get Information

> Regularly this command is used upon receipt of an URC "^SSTN" to request the parameters of the Proactive Command.
> Then the TA is expected to acknowledge the AT^SSTGI response with AT^SSTR to confirm that the Proactive Command has been executed. AT^SSTR will also provide any user information, e.g. a selected menu item.
> The Proactive Command type value specifies to which "^SSTN" the command is related.
> Syntax

> Test Command AT^SSTGI=?
> Response(s)
> ^SSTGI:(list of supported <state>s), (list of supported <cmdType>s)
> OK

> Read Command AT^SSTGI?
> Response(s)
> ^SSTGI: <state>, <cmdType>
> OK

> Write Command AT^SSTGI=<cmdType>
> Response(s)
> OK
> ERROR
> +CME ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <state>(num)

> TC65 Remote-SAT interface states
> 0
> RESET
> 1
> OFF
> 2
> IDLE
> 3
> PAC
> 4
> WAIT

> <cmdType>(num)

> Related Proactive Command