> 5.7 | Shutdown

> If an unexpected shutdown occurs, data scheduled to be written will get lost due to a buffered write access to the flash file system. The best and safest approach to powering down the module is to issue the AT^SMSO command. This procedure lets the engine log off from the network and allows the software to enter a secure state and save all data. Further details can be found in [2].