> 2.4 | ATQ Set result code presentation mode

> This parameter setting determines whether or not the TA transmits any result code to the TE. Information text transmitted in response is not affected by this setting.
> Syntax

> Exec Command ATQ[<n>]
> Response(s)
> If <n>=0:
> OK
> If <n>=1:
> (none)

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <n>(num)(&W)(&V)

> [0](&F)
> DCE transmits result code
> 1
> Result codes are suppressed and not transmitted
> Note

> • | If Java is running, the firmware will ignore the command. Responses will be invalid or result in "ERROR". See also "TC65 Java User's Guide" [4], Section "Configuration of Serial Interface".