> 17.7 | AT^SDLD Delete the 'last number redial' memory

> AT^SDLD deletes all numbers stored in the "LD" memory.
> Syntax

> Test Command AT^SDLD=?
> Response(s)
> OK

> Exec Command AT^SDLD
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Note

> • | Users should be aware that when using this AT command quickly after SIM PIN authentication the SIM data may not yet be accessible, resulting in a short delay before the requested AT command response is returned. See Section 23.1, Restricted access to SIM data after SIM PIN authentication for further detail.