> 4.3.10 | Power Saving Control (PSC)

> The multiplexer of your wireless module supports the power saving control (PSC) messages defined in the GSM 07.10. Nevertheless, the module does not require any settings to be made because power saving is handled automatically (see [1] for details on power saving).
> The power saving control message uses the following type field octet:
> Type:

> Bit 1 | Bit 2 | Bit 3 | Bit 4 | Bit 5 | Bit 6 | Bit 7 | Bit 8
> 1 | C/R | 0 | 0 | 0 | 0 | 1 | 0

> C/R bit: Indicates whether the sequence is a command or a response.
> Length: The length byte contains the value 0 (no value octet) or 1 (one value octet).
> Value octet (Length=1)

> Bit 1 | Bit 2 | Bit 3 | Bit 4 | Bit 5 | Bit 6 | Bit 7 | Bit 8
> P1 | P2 | P3 | P4 | 0 | 0 | 0 | 0

> The P-bits are defining the parameter value.
> In responses:

> Bit 1 | Bit 2 | Bit 3 | Bit 4 | Description
> 0 | 0 | 0 | 0 | Failure
> 1 | 0 | 0 | 0 | Success