> 22.2 | ATS3 Set command line termination character

> The ATS3 command determines the character recognized by the TA to terminate an incoming command line. It is also generated for result codes and information text, along with the ATS4 parameter.
> Syntax

> Read Command ATS3?
> Response(s)
> <n>
> OK

> Write Command ATS3=<n>
> Response(s)
> OK
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <n>(num)(&W)(&V)

> command line termination character
> 000...13(&F)...127
> Notes

> • | Using a value other than the default 13 may cause problems when entering commands.

> • | Whenever you change the setting take into account that the new value has no effect on the URC "^SHUTDOWN".