> 11.23 | Using the GPRS dial command ATD

> Example
> In addition to the GPRS AT commands you can use the "D" command to dial into to the GPRS network.
> There are two GPRS Service Codes for the ATD command: Values 98 and 99.
> Examples:

> ATD*99#
> CONNECT | Establish a connection by service code 99.

> ATD*99*123.124.125.126*PPP*1#
> CONNECT | Establish a connection by service code 99, IP address 123 and L2P = PPP and using CID 1. The CID has to be defined by AT+CGDCONT.

> ATD*99**PPP#
> CONNECT | Establish a connection by service code 99 and L2P = PPP.

> ATD*99***1#
> CONNECT | Establish a connection by service code 99 and using CID 1.

> ATD*99**PPP*1#
> CONNECT | Establish a connection by service code 99 and L2P = PPP and using CID 1. The CID has to be defined by AT+CGDCONT.

> ATD*98#
> CONNECT | Establish a connection by service code 98.

> ATD*98*1#
> CONNECT | Establish an IP connection by service code 98 using CID 1. The CID has to be defined by AT+CGDCONT.