> 2.5 | ATV Set result code format mode

> This command determines the contents of header and trailer transmitted with AT command result codes and information responses. Possible responses are described in Section 2.5.1, Verbose and numeric result codes.
> Syntax

> Exec Command ATV[<value>]
> Response(s)
> OK
> ERROR

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> V.250 |  | - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <value>(num)(&W)(&V)

> [0]
> Information response: <text><CR><LF>
> Short result code format: <numeric code><CR>
> 1(&F)
> Information response: <CR><LF><text><CR><LF>
> Long result code format: <CR><LF><verbose code><CR>