> 8.12.1 | AT^SMONG Cell Info Table

> Example output for AT^SMONG:

> GPRS Monitor
> BCCH G PBCCH PAT MCC MNC NOM TA RAC # Cell #
> 0637 1 - 4 234 05 2 00 0B

> Columns of the cell info table:

> Column | Description
> BCCH | ARFCN of BCCH carrier
> G | GPRS status: 0 GPRS not available in currently used cell 1 GPRS available in currently used cell 2 GPRS attached Note: If the network uses the PBCCH, the correct value can only be displayed if the TC65 is attached.
> PBCCH | If PBCCH is present, indication of ARFCN, else ''-'' or if Frequency Hopping is used ''H''
> PAT | Priority Access Threshold (GSM Rec. 04.08 / 10.5.2.37b) 0 Packet access is not allowed in the cell 1 Spare, shall be interpreted as "000" (packet access not allowed) 2 Spare, shall be interpreted as "000" (packet access not allowed) 3 Packet access is allowed for priority level 1 4 Packet access is allowed for priority level 1 to 2
> MCC | Mobile Country Code
> MNC | Mobile Network Code
> NOM | Network Operation Mode (1...3)
> TA | Timing Advance Value
> RAC | Routing Area Code (as hexadecimal value)