> 9.11 | AT+COLP Connected Line Identification Presentation

> This command refers to the GSM supplementary service COLP (Connected Line Identification Presentation) that enables a calling subscriber to get the connected line identity (COL) of the called party after setting up a mobile originated call. The command enables or disables the presentation of the COL at the TE. It has no effect on the execution of the supplementary service COLR in the network.
> Syntax

> Test Command AT+COLP=?
> Response(s)
> +COLP:(list of supported <n>s)
> OK

> Read Command AT+COLP?
> Response(s)
> +COLP: <n>, <m>
> OK
> ERROR
> +CME ERROR: <err>

> Write Command AT+COLP=[<n>]
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> GSM 07.07 |  | + |  | + | + | + | + | + | + |  |  | - | - | -

> Unsolicited Result Code
> Call response format:
> +COLP: <number>, <type>
> Parameter Description

> <n>(num)

> 0
> Disable - suppress unsolicited result codes
> 1
> Enable - display unsolicited result codes

> <m>(num)

> 0
> COLP not provisioned (no presentation)
> 1
> COLP provisioned
> 2
> Unknown

> <number>(str)

> String type phone number of connected address in format specified by <type>

> <type>(num)

> Type of address octet in integer format; 145 when dialling string includes international access code character "+", otherwise 129.