> 8.18 | AT^SPLW Write an entry to the preferred operators list

> The AT^SPLW write command writes an entry to the SIM list of preferred operators at location number <index>. If <index> is given but <oper> is left out, the entry is deleted. An operator can be only once in the list. Test command returns the whole index range supported by the SIM.
> See also GSM 07.07: AT+CPOL
> Syntax

> Test Command AT^SPLW=?
> Response(s)
> ^SPLW:(list of supported) <index>s
> OK
> ERROR
> +CME ERROR:

> Write Command AT^SPLW=<index>[, <oper>]
> Response(s)
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <index>(num)

> location number

> <oper>(str)

> Operator in numeric format (GSM Location Area Identification number which consists of a 3-digit country code plus a 2- or 3-digit network code).