> 7.26 | AT^SCNI List Call Number Information

> Syntax

> Test Command AT^SCNI=?
> Response(s)
> OK

> Exec Command AT^SCNI
> Response(s)
> ^SCNI: <id>1[,<cs>[,<number>,<type>]]
> ^SCNI: <id>2[,<cs>[,<number>,<type>]]
> [...]
> OK
> ERROR
> +CME ERROR: <err>

> Reference(s) |  | PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> SIEMENS |  | + |  | + | + | + | + | + | + |  |  | - | - | -

> Command Description
> TA returns a list of current calls of ME.
> Parameter Description

> <id>(num)

> call identification number as described in GSM 02.30[19] subclause 4.5.5.1; this number can be used in AT+CHLD command operations
> 1...7

> <cs>(num)

> Call status of respective call number (first parameter)
> 0
> call hold
> 1
> call in progress
> 2
> waiting call

> <number>(str)

> string type phone number in format specified by <type>

> <type>(num)

> type of address octet in integer format; 145 when dialling string includes international access code character "+", 128 when number is restricted otherwise 129
> Note

> • | See also GSM 07.07: AT+CLCC