> 10.2 | AT^SICI Internet Connection Information

> The AT^SICI read command requests the current status of the Internet connection profiles currently defined with AT^SICS.
> The AT^SICI write command displays the status of the specified Internet connection profile. If the connection profile is not defined yet, the command returns a "+CME ERROR" response.
> Syntax

> Test Command AT^SICI=?
> Response(s)
> [^SICI:(list of defined <conProfileId>s)]
> OK

> Read Command AT^SICI?
> Response(s)
> [^SICI: <conProfileId>, <conState>, <numServices>, <conAddr>]
> [^SICI: ...]
> OK

> Write Command AT^SICI=<conProfileId>
> Response(s)
> ^SICI: <conProfileId>, <conState>, <numServices>, <conAddr>
> OK
> ERROR
> +CME ERROR: <err>

> PIN |  | ASC0 | ASC1 | USB | MUX1 | MUX2 | MUX3 |  |  | Charge | Q | Last
> - |  | + | + | + | + | + | + |  |  | - | + | -

> Parameter Description

> <conProfileId>(num)

> Internet connection profile identifier as defined by AT^SICS (<conProfileId>).
> 0...5

> <conState>(num)

> State of the Internet connection profile.
> 0
> Down - Internet connection is defined but not connected.
> 1
> Connecting - A service has been opened and so the Internet connection is initated.
> 2
> Up - Internet connection is established and usable by one or more services.
> 3
> Limited Up - Internet connection is established, but temporarily no network coverage.
> This state applies only to GPRS profiles (it does not occur with CSD).
> 4
> Closing - Internet connection is terminating.

> <numServices>(num)

> Number of services using this Internet connection profile.
> 0...9

> <conAddr>(str)

> Local IP address of the Internet connection profile (empty if no address is associated yet).
> Note

> • | Before opening a service profile based on a connection profile recently used, check with AT^SICI that the previous connection was properly closed. If AT^SICI confirms that the connection profile is in <conState> 0 (Down) the connection profile may be used again.