Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| IM Profile
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package com.siemens.icm.io

Siemens IMP utility classes for accessing the functionality of a wireless module.

See:
Description

Interface Summary
ATCommandListener | The ATCommandListener interface defines the capabilities for receiving unsolicited AT-Events (e.g. like "RING") and changes of the relevant incoming interface signals (RING, DCD and DSR).
ATCommandResponseListener | The ATCommandResponseListenerListener interface defines the capabilities for receiving the response of sending an AT command to a module's AT interpreter.
BearerControlListener | The BearerControlListener interface defines the capabilities for receiving bearer (e.g.
CommConnectionControlLines | The CommConnectionControlLines interface extends CommConnection with the capabilities of actuating on the control lines of a device, which is connected through a CommConnection port.
CommConnectionControlLinesListener | The CommConnectionControlLinesListener interface defines the capability for receiving state changes of the DTR signal.
InPortListener | The InPortListener interface defines the capabilities for receiving value changes at the input ports of the general purpose IO driver (GPIO).
LimitPulseCounterListener | The LimitPulseCounterListener interface defines the capabilities for receiving the indication of a LimitPulseCounter when it has completed counting its number of pulses.

Class Summary
ATCommand | The ATCommand class supports the execution of AT commands on the same way, as it would be done through a serial interface.
ATStringConverter | The ATStringConverter class contains conversion functions for easy conversion between Java strings and GSM or UCS2 encoded strings to be used for parameters of several AT commands via the ATCommand class.
BearerControl | The BearerControl class provides the ability to get bearer state events and to hang-up the bearer.
File | Deprecated. Use javax.microedition.io.FileConnection instead
InPort | This class supports the access and configuration of a port of input pins of the general purpose IO driver (GPIO).
LimitPulseCounter | This class supports the access and configuration to the limit pulse counter of the general purpose IO driver (GPIO).
OutPort | This class supports the access and configuration of a port of output pins of the general purpose IO driver (GPIO).
StartStopPulseCounter | This class supports the access and configuration to the start/stop pulse counter of the general purpose IO driver (GPIO).

Exception Summary
ATCommandFailedException | Signals that a requested device access via the ATCommand class failed.

## Package com.siemens.icm.io Description

Siemens IMP utility classes for accessing the functionality of a wireless module. This package contains utility classes for execution of AT commands and easy access of the flash file system of a wireless module.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| IM Profile
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

Submit a comment or suggestion Version 2.0 of IM Profile Specification
Java is a trademark or registered trademark of Sun Microsystems, Inc. in the US and other countries. Copyright (c) 1993-2002 Sun Microsystems, Inc. 901 San Antonio Road,Palo Alto, California, 94303, U.S.A. All Rights Reserved.