------------------------------------------------------------------------
BE-300.Net "MEM.exe"  Memory residual quantity display program
------------------------------------------------------------------------
<Exception monitoring function>
If the character of exception appears in a debugging output, it will display on the screen lower right.


Whenever it carries out the tap of the taskbar icon,
it changes as follows.

  Window display =>
  Non-window display =>
  Explanation of a non-window display =>
  Un-displaying => Window display....

Changes in the case of a window state.
  It changes as follows on four directions.

<-Work Memory-><-Disk-><-Work Memory Reservation->
------------------ ----------------------------------
^  AvailPhys     Total           Allocate
|  UsingPhys     Free
V  MinAvailPhys  Total Nand
                 Free Nand
                 Total Card
                 Free Card


[Work Memory]
	TotalPhys	Total
	AvailPhys	Remainder
	UsingPhys	Use
	MinAvailPhys	Since MEM is started,The minimum value of AvailPhys

[Disk]
	Total		Main part total size
	Free		Main part free size
	Total Nand	NAND Disk total size
	Free Nand	NAND Disk free size
	Total Card	Storage Card total size
	Free Card	Storage Card free size

[Work Memory Reservation]
	Allocate	By Up/Down is change the size of MEM.

[Un-displaying]
At the time of a window state,
  A work memory, work memory reservation, when not displaying -> [Work Memory]
	AvailPhys / UsingPhys / TotalPhys

  When it is a disk display -> [Disk]
		Free      / Total
		Free Nand / Total Nand
		Free Card / Total Card
